Step 1: Install the LM software, new version download: http://www.yingselectric.com/product_show.asp?id=193
Install the target, please refer the manual page9-10.
Step 2, Install the Weinview HMI software.

Step 3, Both open the PLC program and the HMI program, then download the PLC program to the PowerPro, download the HMI program to the EasyManager. Then have the communication.

Note: MT506T（320*234）in the EasyManager can instead MT506M
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